***Z-BEADS***

***Zirconia Sintering Beads***

Z-Beads Zirconia Sintering Beads provide a better temperature rate when using sintering trays. Because the sintering tray and Z-Beads heat at two different temperature rates, Z-Beads absorb the heat and provide a controlled temperature which helps prevent shrinkage. Zirconia Sintering Beads support crowns, inlays, onlays, veneers, and bridges during the sintering process. Z-Beads can withstand up to 1700 degrees Celsius and are made of high purity zirconia that provide contamination free results for restorations. For best results, use with Vented Sintering Tray.

***Advantages:***

* Helps control temperature of sintering tray
* Perfectly sized at 2mm
* Contamination free firing results
* Controls shrinkage
* High purity
* Withstands up to 1700 degrees Celsius

Size: 200g Jar of 2mm Beads

Item #146

Suggested Retail Price $44.50