***Z-TRAY***

***Vented Sintering Tray and Cover***

Z-Tray Vented Sintering Trays provide a convenient and protective method of sintering. Z-Tray is perfect for sintering crowns, bridges, inlays, onlays, and veneers. This dense, round, ceramic tray provides nearly complete protection from undesired gas vapor condensation on your restoration. Z-Tray used with the sintering cover prevents occasional zirconia discoloring that may otherwise occur due to the heating elements. Having a max service temperature of 1700 degrees Celsius, Z-Tray Vented Sintering Tray maintain good thermal shock and can withstand both a fast heating rate for zirconia and a slow heating rate for long-span bridgework or complex cases. For best results, use with zirconia sintering beads.

***Advantages:***

* Easily used for fast and slow heating rates
* Contamination free firing results
* Good thermal shock
* Resistant to cracking
* Withstanding up to 1700 degrees Celsius

Size: 100mm tray with cover

Item #144

Suggested Retail Price $49.50