***WONDERPEG***

***Instant Firing Support***

This Instant Soldering and Firing Support is used to support crowns, jackets, and veneers on a firing peg during the kiln process. No mixing or pre-drying time is required with Wonderpeg Instant Firing Support. Working as a heat shield, Wonderpeg has zero firing distortion and works well when soldering structures. For temperatures 400°C to 1300°C. Convenient 10cc syringe provides easy application.

***ADVANTAGES:***

* For use with e.max & Lava crowns
* No pre-drying time
* Zero firing distortion
* Does not contaminate
* For temperatures from 400°C - 1300°C



**Item# 2010**

Suggested Retail: $7.50